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EK-2

	Yüksek Basınçlı Sodyum
	Bütün çeşitleri ve sınıfları.

	Metal Halojenur
	Bütün çeşitleri ve sınıfları.

	Endiksiyon Aydınlatmalı
	Bütün çeşitleri ve sınıfları.

	Boru Şeklinde Fleurosan
	26 mm çapında (T8) lambalar,
16 mm çapında (T5) ve 11 W üzerinde sınıflandırılmış yüksek verimli kumanda dişlisine sahip  lambalar ve

(T12) lineer 2400 mm uzunluğunda fleurosan lambalar.

	Kompakt Fleurosan
	11W üzerindeki bütün sınıfları ve enerji verimliliği 50 lümen/devreWatt’tan büyük olan bütün çeşit ve sınıfları.

	Diğer
	Lambanın enerji verimliliği 50 lümen/devreWatt ‘tan büyük olan bütün çeşit ve sınıfları. 


 Genel Aydınlatma İçin Uygun  Aydınlatma Kaynakları
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BEP ile ilgili Türk Standardları Listesi
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	Binalarda Isı Yalıtım 
	2008

	TS EN ISO 10211-1
	Bina İnşaatlarında Isıl Köprüler - Isı Akışları ve Yüzey Sıcaklıkları - Bölüm 1: Genel Hesaplama Metotları
	2000
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	2001
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	2006
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	Bacalar – Isı ve akışkan dinamiği hesaplama metotları – Bölüm 2: Birden çok ısıtma tertibatına bağlı bacalar
	2006

	TS 2192
	Kalorifer Tesisatı Yerleştirme Kuralları
	1976

	TS EN 378-1
	Soğutma sistemleri ve ısı pompaları - Güvenlik ve çevre kuralları - Bölüm 1: Temel kurallar, tarifler, sınıflandırma ve seçim kriterleri
	2007

	TS EN 378-2
	Soğutma sistemleri ve ısı pompaları - Güvenlik ve çevre kuralları- Bölüm 2: Tasarım, yapım, deney, işaretleme ve dokümantasyon
	2004
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	Soğutma Sistemleri ve Isı Pompaları - Güvenlik ve Çevre Kuralları- Bölüm 3: Tesis Yeri ve Personel Koruma
	2002

	TS EN 378-4
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	2001
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	2002
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	1998
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	Havalandırma ve İklimlendirme Tesislerini Yerleştirme Kuralları
	1979

	TS EN 1507 
	Havalandırma-Binalarda-Kanal Şebekesi-Dikdörtgen Enkesitli Sac Metal Hava Kanalları-Dayanım ve Sızdırmazlık-Özellik ve Deneyler
	 
2006 
 

	TS EN 12237
	Binalarda havalandırma – Kanal şebekesi – Dairesel sac metal kanallar – Dayanım ve sızdırmazlık
	2006

	TS EN 14336
	Isıtma sistemleri - Binalar için - Su esaslı ısıtma sistemlerinin tesisi ve işletmeye alınması
	2007

	TS EN 26
	Ani Su Isıtıcılar (Şofbenler)-Gaz Yakan, Atmosferik Brülörlü
	2006

	TS EN 89
	Isıtıcılar – Gaz yakan – Ev tipi – Sıcak su üretimi için depolu su ısıtıcılar
	2008

	TS EN 12975-1
	Isıl güneş enerji sistemleri ve bileşenleri-Güneş enerjisi kolektörleri-Bölüm 1:Genel Kurallar
	2008

	TS 3817
	Güneş Enerjisi - Su Isıtma Sistemlerinin Yapım Tesis ve İşletme Kuralları
	1994

	 
TS EN 215 
	Radyatör vanaları – termostatik –Özellikler ve deney metotları
	2007

	TS EN 832 
	Binaların Isıl Performansı – Meskenlerde Isıtma Amacıyla Kullanılan Enerjinin Hesaplanması
	2007
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	Isı Maliyet Bölüştürücüleri - Radyatör Isı Tüketiminin Belirlenmesinde Kullanılan - Elektrik Enerjisi İle Çalışan
	1997

	TS 4041 
	Kazanlar- Anma Isı Gücü Ve Verim Deneyleri Esasları
	1983

	TS ISO 9459-1 
	Güneş Enerjisiyle Isıtma-Konut Su Isıtma Sistemleri-Bölüm 1:İç Ortam Deney Metotları Kullanılarak Performans Değerlendirme İşlemi
	1999

	TS ISO 9459-2 
	Güneş Enerjisi Konut Su Isıtma Sistemleri Bölüm 2: Sadece Güneş Enerjili Sistemlerin Yıllık Performans Tahmini Ve Sistem Performans Karekteristikleri İçin Dış Ortam Deney Metodu
	2000

	TS ISO 9459-3 
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	1999
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 EK- 8b. BEP ile ilgili Avrupa Standardları Listesi
	EN 12170
	Heating systems in buildings - Procedure for the preparation of documents for operation, maintenance and use - Heating systems requiring a trained operator
	2002

	EN 12171
	Heating systems in buildings - Procedure for the preparation of documents for operation, maintenance and use - Heating systems not requiring a trained operator
	2002

	EN 12828
	Heating systems in buildings - Design for water-based heating systems
	2003

	EN 12831
	Heating systems in buildings - Method for calculation of the design heat load  
	2003

	EN 14336
	Heating Systems in buildings - Installation and commissioning of the water based heating systems  
	2004

	EN 15240
	Ventilation for Buildings - Energy performance of buildings : Guidelines for the inspection of air-conditioning systems.
	2007

	EN 15243
	Ventilation for Buildings - Calculation of room temperatures and of load and energy for buildings with room conditioning systems
	2007

	EN 15316-1 
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 1: General
	2007

	EN 15316-2-1
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies : Part 2.1: Space heating emission systems
	2007

	EN 15316-2-3
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 2-3: Space heating distribution systems
	2007

	EN 15316-3-1
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 3: Domestic hot water systems
	2007

	EN 15316-3-2
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 3-2: Domestic hot water systems, distribution  
	2007

	EN 15316-3-3
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 3-3: Domestic hot water systems, generation
	2007

	EN 15316-4-3
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 4-3: Heat generation systems, thermal solar systems
	2007

	EN 15316-4-4 
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 4-4: Heat generation systems, building-integrated cogeneration systems
	2007

	EN 15316-4-5 
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 4-5: Space heating generation systems, the performance and quality of district heating and large volume systems
	2007

	EN 15316-4-6
	Heating systems in buildings - Method for calculation of system energy requirements and system efficiencies - Part 4-6: Heat generation systems, photovoltaic systems
	 

	EN 15377-3 
	Design of embedded water based surface heating and cooling systems
	2007 

	EN 15378 
	Energy performance of buildings: Inspection of boilers and heating systems
	 

	EN 15217 
	Energy performance of buildings - Methods of expressing energy performance and for energy certification of buildings
	2007

	EN 12464-1 
	Light and lighting - Lighting of work places - Part 1: Indoor work places
	2002

	EN 12464-2 
	Light and lighting - Lighting of work places - Part 2: outdoor work places  
	2007

	EN 12665 
	Light and lighting - Basic terms and criteria for specifying lighting requirements
	2002

	EN 13032-1 
	Light and lighting - Measurement and presentation of photometric data of lamps and luminaires - Part 1 : Measurement and file format
	2004

	EN 13032-1/AC:2005 
	Light and lighting - Measurement and presentation of photometric data of lamps and luminaires - Part 1 : Measurement and file format 
	2005

	EN 13032-2 
	Light and lighting - Measurement and presentation of photometric data of lamps and lumlinaires - Part 2 : Presentation of data for indoor and outdoor work places
	2005

	EN 13032-2/AC:2007 
	Light and Lighting - Measurement and presentation of photometric data of lamps and luminaires- Part 2 : Presentation of data for indor and outdoor work places  
	2007

	EN 15193 
	Energy performance of buildings - Energy requirements for lighting  
	2007

	EN 12097 
	Ventilation for buildings - Ductwork - Requirements for ductwork components to facilitate maintenance of ductwork systems
	2006

	EN 12220 
	Ventilation for buildings - Ductwork - Dimensions of circular flanges for general ventilation
	1998

	EN 12236 
	Ventilation for buildings - Ductwork hangers and supports - Requirements for strength 
	2002

	EN 12237 
	Ventilation for buildings - Ductwork - Strength and leakage of circular sheet metal ducts 
	2003

	EN 12238 
	Ventilation for buildings - Air terminal devices - Aerodynamic testing and rating for mixed flow application
	2001

	EN 12239 
	Ventilation for buildings - Air terminal devices - Aerodynamic testing and rating for displacement flow applications  
	2001

	EN 12589
	Ventilation for buildings - Air terminal units - Aerodynamic testing and rating of constant and variable rate terminal units   
	2001

	EN 12599  
	Ventilation for buildings - Test procedures and measuring methods for handing over installed ventilation and air conditioning systems
	2000

	EN 12792 
	Ventilation for buildings. Symbols, terminology and graphical symbols
	2003

	EN 13030 
	Ventilation for buildings - Terminals - Performance testing of louvres subjected to simulated rain  
	2001

	EN 13053 
	Ventilation for buildings - Air handling units - Ratings and performance for units, components and sections
	2006

	EN 13141-1 
	Ventilation for buildings - Performance testing of components/ products for residential ventilation - Part 1. Externally and internally mounted air transfer devices
	 2004 
 

	EN 13141-2
	Ventilation for buildings - Performance testing of components/products for residential ventilation - Part 2. Exhaust and supply air terminal devices 
	2004

	EN 13141-3 
	Ventilation for buildings - Performance testing of components/products for residential ventilation - Part 3. Range hoods for residential use
	2004

	EN 13141-4
 
	Ventilation for buildings – Performance testing of components/products for residential ventilation - Part 4. Fans used in residential ventilation systems
	2004 

	EN 13141-5 
	Ventilation for buildings - Performance testing of components/products for residential ventilation - Part 5. Cowls and roof outlet terminal devices   
	2004

	EN 13141-6 
 
	Ventilation for buildings - Performance testing of components/products for residential ventilation - Part 6. Exhaust ventilation system packages used in a single dwelling   
	2004

	EN 13141-7
	Performance testing of components/products for residential ventilation - Part 7: Performance testing of a mechanical supply and exhaust ventilation units (including heat recovery) for mechanical ventilation systems intended for single family dwellings   
	2004

	EN 13141-8 
	Ventilation for buildings - Performance testing of components/products for residential ventilation - Part 8: Performance testing of un-ducted mechanical supply and exhaust ventilation units for mechanical ventilation systems   
	2006

	EN 13142 
	Ventilation for buildings – Components / products for residential ventilation – Required and optional performances characteristics  
	2004 
 

	EN 13180 
	ventilation for buildings - Ductwork - Dimensions and mechanical requirements for flexible ducts. 
	2001

	EN 13181 
	Ventilation for buildings - Terminals - Performance testing of louvres subject to simulated sand
	2001

	EN 13182
	Ventilation for buildings - Instrumentation requirements for air velocity measurements in ventilated spaces
	2002

	EN 13264 
	Ventilation for buildings - Terminals - Floor mounted air terminal devices - Tests for structural classification 
	2001

	EN 13403 
	Ventilation for buildings. Non metallic ducts. Ductwork made from insulation ductboards  
	2003 

	EN 13465 
	Ventilation for buildings - Calculation methods for the determination of air flow rates in dwellings  
	2004

	EN 13829 
	Thermal performance of buildings - Determination of air permeability of buildings - Fan pressurization method (ISO 9972:1996, modified)  
	2001 

	EN 14134 
 
	Ventilation for buildings - Performance testing and installation checks of residential ventilation systems  
	2004 
 

	EN 14239 
	Ventilation for buildings - Ductwork - Measurement of ductwork surface area  
	2004

	EN 14240 
	Ventilation for buildings - Chilled ceilings - Testing and rating   
	2004

	EN 14277 
	Ventilation for buildings - Air terminal devices - Method for airflow measurement by calibrated sensors in or close to ATD/Plenum boxes   
	2006

	EN 14518 
	Ventilation for buildings - Chilled beams - Testing and rating of passive chilled beams  
	2005

	EN 1505 
	Ventilation for buildings - Sheet metal air ducts and fiffings with rectangular cross section - Dimensions   
	1997

	EN 1506 
	Ventilation for buildings - Sheet metal air ducts and fittings with circular cross-section - Dimensions
	  1997

	EN 1507 
	Ventilation for buildings - Sheet metal air ducts with rectangular section - Requirements for strength and leakage   
	2006

	EN 15239 
 
	Ventilation for buildings - Energy performance of buildings - Guidelines for inspection of ventilation systems  
	2007

	EN 15242 
	Ventilation for buildings - Calculation methods for the determination of air flow rates in buildings including infiltration
	2007

	EN 15251 
	Indoor environmental input parameters for design and assessment of energy performance of buildings addressing indoor air quality, thermal environment, lighting and acoustics    
	2007

	EN 1751 
	Ventilation for buildings - Air terminal devices - Aerodynamic testing of dampers and valves 
	1998

	EN 1886 
	Ventilation for buildings - Air handling units - Mechanical performance   
	1998

	EN 24185
	Measurement of liquid flow in closed conduits - Weighing method 
	 

	EN 779
	Particulate air filters for general ventilation - Determination of the filtration performance 
	 

	EN ISO 5167-1
	Measurement of fluid flow by means of pressure differential devices inserted in circular cross-section conduits running full - Part 1: General principles and requirements
	 

	EN 15232 
	Energy performance of buildings - Impact of Building Automation, Controls and Building Management 
	2007

	EN 15255 
 
	Thermal performance of buildings - Sensible room cooling load calculation - General criteria and validation procedures   
	2007

	EN ISO 13791
	Thermal performance of buildings - Calculation of internal temperatures of a room in summer without mechanical cooling - General criteria and validation procedures 
	2004

	EN ISO 13792
	Thermal performance of buildings - Calculation of internal temperatures of a room in summer without mechanical cooling - Simplified methods
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ISI YALITIMI UYGULAMASI HİZMET SÖZLEŞMESİ


Taraflar


Madde 1- Aşağıda isim (unvan) ve adresleri yazılı bulunan Müşteri ile Uygulayıcı Firma arasında “Uygulama Sözleşmesi” yapılmıştır. Taraflar bundan sonra  “Müşteri“ ve “Yüklenici“ olarak anılacaktır.

TARAFLAR 

Müşteri     

Adı, soyadı, unvanı


: ..........................................................................         






  ……………………………………………….

Adresi




: ...........................................................................

Tel, faks, e-posta


: ...........................................................................

Yüklenici

Adı, soyadı, unvanı


: ............................................................................






  …………………………………………………

Adresi




: .............................................................................

Tlf, faks, e-posta


: ..............................................................................

İrtibat Bilgileri 


           : ………………………………………………….

(Adres, Tlf, faks, e-posta)

Kapsam

Madde 2- ……………..………………………………..…..………….. adresinde toplam …………………………………..……….. bağımsız bölümden oluşan yapıya, Binalarda Enerji Performansı Yönetmeliğine göre hazırlanmış olan ısı yalıtım projesinin uygulanması ve enerji kimlik belgesinin alınması işidir.

Süre

Madde 3- Sözleşme konusu işin teslim süresi, sözleşmenin imzalandığı tarihten itibaren ………….….. takvim günü olup, bu süre Müşteri tarafından kabul edilen mücbir sebepler dışında uzatılamaz.

Uygulamalar

Madde 4-(1) Uygulamalar, Binalarda Enerji Performansı Yönetmeliği doğrultusunda, Isı yalıtım raporuna uygun ve TS 825 Standardının EK-E’sinde yer alan veya Ulusal Teknik Onay kuruluşlarından onay almış malzemeler kullanılarak yapılacaktır.
(2) Uygulama yapılırken, (Değişik ibare:RG-19/2/2022-31755) Çevre, Şehircilik ve İklim Değişikliği Bakanlığı (Mesleki Hizmetler Genel Müdürlüğü) web sitesinde yayınlanan Isı Yalıtım Uygulama Kılavuzu veya üretici firma dokümanlarına dikkat edilecektir. 

(3) Kullanılacak yapı ve yalıtım malzemeleri için Yapı Malzemeleri Yönetmeliği çerçevesinde, Yapı ve Yalıtım Malzemelerinin CE veya G uygunluk işareti ve uygunluk beyanı veya belgesi alması zorunludur.

Enerji Kimlik Belgesi

Madde 5-Yüklenici, Uygulamanın tamamlanmasını müteakip ısı/sıcaklık görüntüleme cihazı ve ısıl geçirgenlik ölçüm cihazı ile belgelendirerek, yetkili kuruluş aracılığıyla binaya enerji kimlik belgesinin oluşturulmasını sağlayacaktır.
Müşterinin Sorumlulukları

Madde 6- Yükleniciye çalışma imkanı ile uygulama süresince gerekli elektrik ve su ihtiyaçlarını karşılayacaktır.
Yüklenicinin Sorumlulukları

Madde 7-(1)- Yüklenici uygulamaların proje, fen ve sanat kurallarına uygun olarak yapılmasından sorumlu olup, bu kapsamda çalıştırdığı ustaların Mesleki Yeterlilik Kurumu tarafından yetkilendirilmiş sınav ve belgelendirme kuruluşlarından alınmış “Isı Yalıtımcısı” olduğuna dair Mesleki Yeterlik Belgelerini beyan edecektir.

(2)- Yüklenici, ilgili mevzuat uyarınca iş sağlığı ve güvenliği ile çevre ve sağlık şartları ile ilgili her türlü tedbiri alacaktır. 

(3)- Uygulamalar nedeniyle çıkacak tüm moloz ve atık malzemeyi ilgili belediyece gösterilen yerlere ve uygun şekilde taşınarak boşaltılmasını sağlayacaktır.

(4)- Yüklenici, sözleşme konusu işle ilgili yapacağı nakliye ve imalatın her aşamasındaki hasarlardan sorumlu olacaktır.

Garanti

Madde 8- Yüklenici, sözleşme konusu işlerin Müşteri tarafından kesin kabulünün yapıldığı tarihten itibaren beş (5) yıl süreyle malzeme ve uygulama hatalarından sorumludur.

YÜKLENİCİ




MÜŞTERİ

”

EK-10 (Ek:RG-19/2/2022-31755) (Değişik:RG-24/6/2025-32936) 
Ön Hesap Sonuç Formu
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Yapi ruhsatina esas projeye ve eklerine gére diizenlenmis olup, Enerji Kimlik Belgesi yerine kullanilamaz.

“Muhtemel Yapi Ruhsat Tariini fade Eder. EK: Bina ve Mekanik Sistem Bilgileri (1 Sayfa)





