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	GAZİRAY BANLİYÖ TREN SETLERİ İÇİN TİP ONAY VE TESCİL KRİTERLERİ

	NO
	STANDARD
	UYGUNLUK DEĞERLENDİRME KONUSU

	1
	EN ISO 9001
	Quality Systems- Quality Assurance Model in Design, Improvement,
Manufacturing, Fa-cility and Service

	2
	EN 12082
	Railway applications. Axleboxes. Performance testing

	3
	EN 12663
	[bookmark: _GoBack]Railway applications- Structural requirements of railway vehicle bodies

	4
	EN 13260
	Railway applications - Wheelsets and bogies – Wheelsets – Product requirements

	5
	EN 13261
	Railway applications - Wheelsets and bogies - Axles - Product requirements

	6
	EN 13262
	Railway applications - Wheelsets and bogies - Wheels - Product requirements

	7
	EN 13272
	Railway applications - Electrical lighting for rolling stock in public transport
systems

	8
	EN 13452-1
	Railway applications — Braking — Mass transit brake systems — Part 1:
Performance requirements

	9
	EN 13452-2
	Railway applications — Braking — Mass transit brake systems — Part 1: Test
methods

	10
	EN 13749
	Railway applications ― Wheelsets and bogies ―. Method of specifying the
structural requirements of bogie frames

	11
	EN 14363
	Railway applications - Testing for the acceptance of running characteristics of
railway vehicles

	
12
	
EN 14535-1
	Railway applications - Brake discs for railway rolling stock - Part 1: Brake discs pressed or shrunk onto the axle or drive shaft, dimensions and quality requirements

	13
	EN 14535-2
	Railway applications - Brake discs for railway rolling stock - Part 2: Brake discs
mounted onto the wheel, dimensions and quality requirements

	14
	EN 14750-1
	Railway applications - Air conditioning for urban and suburban rolling stock -
Part 1: Comfort parameters

	15
	EN 14750-2
	Railway applications - Air conditioning for urban and suburban rolling stock -
Part 2: Type tests

	16
	EN 14752
	Railway applications. Bodyside entrance systems

	17
	EN 14813-1
	Railway applications - Air conditioning for driving cabs - Part 1: Comfort
parameters

	18
	EN 14813-2
	Railway applications - Air conditioning for driving cabs - Part 2: Type tests

	19
	EN 15085
	Railway Applications - Welding of Railway Vehicles and Components

	20
	EN 15085-2
	Management System for Welding Operations of Railway Vehicles and
Components

	21
	EN 15595:2018
	Railway applications. Braking. Wheel slide protection

	22
	EN 45545-1
	Railway applications. Fire protection on railwayvehicles. General

	23
	EN 45545-2
	Railway applications.Fire protection on railway vehicles. Requirements for fire
behaviour of materials and components

	24
	EN 45545-3
	Railway applications.Fire protection on railway vehicles. Fire resistance
requirements for fire barriers






	
25
	
EN 45545-4
	Railway applications.Fire protection on railway vehicles. Fire safety requirements for electrical equipment including that of trolley buses, track guided buses and magnetic levitation vehicles

	
26
	
EN 45545-5
	Railway applications.Fire protection on railway vehicles. Fire safety requirements for electrical equipment including that of trolley buses, track guided buses and magnetic levitation vehicles

	27
	EN 45545-6
	Railway applications.Fire protection on railway vehicles. Fire control and
management systems

	28
	EN 50121
	Railway Applications - Electromagnetic Compatibility

	
29
	
EN 50126-1
	Railway Applications - The specification and demonstration of reliability, availability, maintainability and safety (RAMS) - Part 1: Basic requirements

	
30
	
EN 50126-2
	Railway Applications.The Specification and Demonstration of Reliability, Availability, Maintainability and Safety (RAMS).Part 2. Systems approach to safety

	31
	EN 50153
	Railway applications-Rolling stock-Protective provisions relating to electrical
hazards

	32
	EN 50155
	Railway applications-Electronic equipment used on rolling stock.

	33
	EN 50215
	Railway applications. Testing of rolling stock after completion of construction
and before entry into service

	34
	EN 50206-1
	Railway applications. Rolling stock. Pantographs. Characteristics and tests

	35
	EN 50264-1
	Railway applications. Railway rolling stock power and control cables having
special fire performance. General requirements

	36
	EN 50264-2
	Single Core Cables

	37
	EN 50264-3
	Multi Core Cables

	38
	EN 50305
	Fire Testing Methods

	39
	EN 50306
	Special Fire Performance

	40
	EN 50343
	Installation of Cabling

	
41
	
EN 50355
	Railway Applications - Railway Rolling Stock Cables Having Special Fire Performance - Guide to use Provides guidance on the safe use of thin walled and standard walled cables

	42
	EN 60947-2:2017
	Low-voltage switchgear and controlgear. Circuit-breakers

	43
	EN ISO 3095
	Railway applications — Acoustics —. Measurement of noise emitted by vehicles
moving on the rail

	44
	EN ISO 3381
	Railway applications — Acoustics. Measurement of noise inside railbound
vehicles

	45
	IEC 60068
	Environmental Tests

	46
	IEC 60076
	Power transformers

	47
	IEC 60349-2
	Electric traction - Rotating electrical machines for rail and road vehicles

	48
	IEC 60623
	Secondary cells and batteries containing alkaline or other non-acid electrolytes -
Vented nickel-cadmium prismatic rechargeable single cells.

	49
	EN 61287-1
	Railway applications - Power converters installed on board rolling stock - Part 1:
Characteristics and test methods

	50
	IEC 61373
	Railway application- Rolling stock equipment- Shock and Vibration tests

	51
	IEC 61375-1
	Electric railway equipment - Train bus - Part 1: Train Communication network

	52
	UIC 540
	Brakes-Air Brakes for freight trains and passenger trains




	53
	UIC 541-03
	Brakes – Disc Brakes and applications – General requirements for approving the brake pads

	54
	UIC 541-4
	Brakes - Brakes with composition brake blocks

	55
	UIC 541-5
	Brakes - electropneumatic brake - electropneumatic emergency brake override

	56
	UIC 544-1
	Brakes – Braking Performance

	57
	UIC 545
	Brakes - Inscriptions, marks and signs

	58
	UIC 560
	Doors, footboards, windows, steps, handles and handrails of coaches and luggage
vans

	59
	UIC 564-1
	Coaches - wındows made from safety glass

	60
	TS 12694
	Railway vehicles- Passenger coaches- Indications for the layout of coaches
suitable for conveying disabled passengers in their wheelchairs

	61
	UIC 641
	Railway Application - Rolling Stock - Conditions to be fulfilled by automatic vigilant devices used in International traffic

	62
	UIC 651
	Layout of driver's cabs in locomotives, railcars, multiple unit trains and driving
trailers.
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